New Features – OpenVBX 09/07/2011

The following features have been added to the OpenVBX package:

* Fixed a redirect bug. The VBX no longer incorrectly redirects users to 404 pages.
* Fixed bug in Twilio client. 60 seconds after the user has been “inactive”, the Twilio client is no longer able to be called for that user. This prevents calling the Twilio client if the user has closed their browser. (This also works for the new Phono client.)
* Added support for the Tropo API. You can now add a “Tropo API account” on the system settings page, and from the installer. Either a Tropo or Twilio account is required. Included in the new Tropo API additions are:
  1. Support for Tropo domestic and international phone numbers, on the “numbers” page.
  2. All applets in the “flows” page now support Tropo JSON as well as Twiml. Any number can be assigned any flow – so a tropo number and a twilio number can both be assigned the same flow.
  3. Support for existing Tropo numbers & applications. If the user prefers to set up their numbers initially in Tropo.com, the application will see these numbers and they can be assigned a flow within the application.
  4. Recordings, and Voicemail, as well as outbound dialing with Tropo.
* Several theme changes. The OpenVBX logo has been modified to include both the Tropo and Twilio logo. If only one of the accounts is active, only that logo will show in the VBX logo – so if a user only has a Twilio account, only the Twilio logo will show, and vice versa. Other minor theme changes:
  1. Several pages in the System Settings tabs have been reworked. Notibly the API accounts page, which now has each API accounts logos.
  2. Step 3 of the installation has been reworked.
  3. Several Twilio-specific content has been changed to be more ambiguous.
* Added support for “Phono” browser phone, in addition to the Twilio Client. Any non-Twilio based numbers will use the new Phono browser phone.
* VoiceVault specific pieces. You can now configure a VoiceVault API account, which improves the password reset system with the security of voice biometrics.